**Safe Work Method Statement**

**Form 007.2**

**Safe Work Method Statement (Part 1)**

|  |  |
| --- | --- |
| **Job: MARQUEE SET-UP** | **Document Reference** |
| **Department:** **Section: HOSPITALITY****Work Area: RACECOURSE GROUNDS** | **No:** |
| **Revision Date:****Manager’s Approval:****Manager’s Name:** |
| **Key Safety Plant / Equipment / (including P.P.E.)** | **Safety Checks / Hazardous Substances** |
| * PPE: enclosed footwear / steel capped boots / gloves
* Adequate number of staff
* Approved hammer
* Forklift
 | * Physical inspection of marquee, poles and ropes
* Physical inspection of hammer
* Physical inspection of worksite for power lines, foreign matter & verify location/existence of in-ground services
* Check forklift – safety guards in place
 |
| **Codes of Practice Legislation: Applicable to Work? Y/N** **If Yes, state:** | **External Considerations**Location/proximity of overhead & in-ground services |
| **Person/s required to carry out work** | **Duties & Responsibilities** | **Qualifications / Experience / Training required to do work** |
| Forklift operatorAdequate number of staff to assist with supervisor in attendance | Forklift for unloading marqueeSupervisor to ensure marquee is erected correctly and that staff follow instructions | Forklift operations licenseFollow instructions with marquee Ensure a staff member has experience with marquee erection and use of equipment |

|  |  |
| --- | --- |
| **SAFE WORK METHOD STATEMENT (PART 2)**  | **Document Reference:** |
| **Job: MARQUEE SET-UP** | **No:** |
| **Procedure (in steps)**  | **Possible Hazards in Executing Procedure** | **Key Safety Controls & Associated Procedures** |
| Unloading marquee and unfold | Muscle strain and back injury | Trained staff to unload |
| Check for vermin / spiders | Possible bites and stings | Wear gloves, unfold with caution. Remove vermin if safe to do so |
| Check site  | Un-even ground surface / power lines | Verify no overhead power lines in proximityVerify no underground services/cables and water pipes; sand to fill surface area |
| Check marquee ropes and pegs | Collapse on workers causing injury | Visual inspection to detect any weakness |
| Staff wearing correct PPE |  |  |
| Instruct all staff in marquee set up | Injury to workers | Ensure all staff follow instructions from supervisor and not interfere with safe erection of marquee |
| Assemble initial pegs | As above and injury from mis-hits with hammer | As AboveMinimum 4 people for 3m x 3 m and increase by 2 people per 3 meter extension |
| Assemble centre pole and install | As aboveEye injury from metal  | wear goggles |
| Lift actual marquee top into place and secure |  |  |
| On completion check security of marquee / ropes / pegs and poles | If not erected correctly and secured, marquee may fall and injure people | Supervisor to check |
| Ensure excess rope is tied off | Workers and public may becomes entangled and injured | Make sure rope ends are not left trailing on ground |
| Ensure ground pegs are flagged | If pegs not highlighted or flagged, public may trip or fall | Ensure flags are bright and visible supervisor to check |
| **Procedure (in steps)**  | **Possible Hazards in Executing Procedure** | **Key Safety Controls & Associated Procedures** |
| Clean up area | Trips and falls | Observation / warning signs |
| If erected a day before, supervisor / appointed staff member to re check ropes / poles / pegs on race day |  |  |
| Lash-down (storm) | Structure collapses or becomes airborne/ impalement hazard | Prior to onset of stormy weather and/or imminent severe weather, inspect structure & tightly lash-down ropes/poles. Alternatively, evacuate area if storm is of severe intensity. |