**Safe Work Method Statement**

**Form 007.2**

**Safe Work Method Statement (Part 1)**

|  |  |
| --- | --- |
| **Job: OPERATION OF OUTFRONT MOWER** | **Document Reference** |
| **Department: TRACKS & SURROUNDS MAINTENANCE****Section: MAINTENANCE / GROUNDS****Work Area: ALL GRASSED AREAS** | **No:** |
| **Revision Date:****Manager’s Approval:****Manager’s Name:** |
| **Key Safety Plant / Equipment / (including P.P.E.)** | **Safety Checks / Hazardous Substances** |
| * Safety glasses, earmuffs, sun protection, steel cap boots, gloves, garbage grabber
 | * Fuel leaks, battery leaks, coolant leaks, tyres, brakes, seatbelt, safety cut off.
 |
| **Codes of Practice Legislation: Applicable to Work? Y/N****If Yes, state:** | **External Considerations** |
| **Person/s required to carry out work** | **Duties & Responsibilities** | **Qualifications / Experience / Training required to complete work** |
| Track appointed operator | Mowing of tracks and surrounds as per instruction | Cert III Turf Knowledge of Operations ManualOn the Job training |

|  |  |
| --- | --- |
| **SAFE WORK METHOD STATEMENT (PART 2)** | **Document Reference:** |
| **Job: OPERATION OF OUTFRONT MOWER** | **No:** |
| **Procedure (in steps)** | **Possible Hazards in Executing Procedure** | **Key Safety Controls & Associated Procedures** |
| All guards in place  | Lacerations, muscle strain | Level clean surface with safe lighting.PPE (gloves) as requiredEnsure machine is switched-off & key removed |
| Safety belts, tyres and all fittings | Manual strain | Correct manual handling techniquesPPE (gloves as required)Ensure machine is switched-off & key removed |
| Check blades for correct type and attachment and conditions | Manual strain | Correct manual handling techniquesPPE (gloves as required)Ensure machine is switched-off & key removed |
| All fittings, fuels, fluids / leaks | Fire / explosion / acid burns | PPE – gloves, glasses, clothingIf leaks, tag and notify |
| Refuel mower as required  | Fuel spillageFire & explosion | Ensure refuelling is undertaken in area with containment bunding/berm, away from drains & spill kit is available. Wear protective clothing as necessary.Ref: Refueling Procedure. Keep clear of ignition sources including mobile phones & microwave ovens. |
| Conduct inspection of site | Foreign materials, debris, rocks, sprinklers, soft areas | Approved gloves, container for sharps, garbage grabber |
|  | Sun burn, fatigue, dehydration | PPE, hat sunscreen, water bottle |
|  | Insect bites, vermin, spider | PPE, call WIRES, notify supervisor |
| **Procedure (in steps)** | **Possible Hazards in Executing Procedure** | **Key Safety Controls & Associated Procedures** |
| Operations | Ensure area does not exceed maximum permissible slope | Check Operations manualEnsure ROPS system in-place & structurally sound |
| Turn-off motor and lock | Prevent unauthorised use of equipment | Ensure keys removed from ignition & securely stored |
| Cleaning of equipment | Slipping and falls | Well-drained areaPPE (gloves as required)Ensure machine is switched-off & key removed |
| Cleaning of PPE | Damage/excessive wear & tear | Replace as required |
| Fill out data book / application diary | None | Weather – control process if necessary |